8 malefemale

204RET^{br} B -204VDC Lamp includes base and wired socket. bu A COMPARISON LAMP

PHOTRON MODEL P209 (MODIFIED)

CALIBRATION LAMP, COPPER HOLLOW CATHODE 4mA TO POWER SUPPLY FOR female male

+24V^w 1 COPPER* 2^{gn} 7

A A* male female

OUTPUT 5 11

PHASE A 1

PHASE A* B

2 FLIP MIRROR MOTOR

PHASE B 14

PHASE B* B* 15 NC NC 3 6

FROM 6K8

OUTPUT: ACTIVE LOW TTL

*: COMPLIMENTARY PHASE

NC: NO CONNECTION.

MODEL IM483 FOR AXIS 5)

IMS STEPPER MOTOR DRIVER

5 (COMPUMOTOR MODEL 6K8 AND

TO WIRO 8-AXIS CONTROLLER NO C NC

FOUR MICROSWITCHES

Filter slide is manually activated.

C: Common. NC: Normally Closed. NO: Normally Open

TO 6K8

TRIG: ACTIVE LOW TTL NO male female C

24RET^{bk}

2 NC

TRIG12

4^{bu}11

TRIG11 4^{gn}

TRIG10 3^y

TRIG9^r 5 ISOGND^{bk} 12 +24V^w

9 NO C NC

3 NO C NC

SHUTTER 2 NC: NO CONNECTION.

FROM CONTROLLER

*: ACTIVE LOW TTL - 6 - 5 VOLTS female male 200 OHMS

+4.4 VDC + H AND TO AUXILIARY POWER SUPPLY 2 + 7 E DUAL READOUT CONTROLLER 1 D CAMERAS, INC.

NC 8 B ASTRONOMICAL RESEARCH 14

SHUTTER* A

TO 6 PIN HI-ROSE CONNECTOR ON

1 CLOSED WHEN ENERGIZED

F E D C B A _______

+24V

+24V

bk r w gn clr Belden_8723

Doc. Number

Number: 1.0Rev. :

Wyoming Infrared Observatory

Root.sch

File:

Project:

Title: Long Slit Spectrograph

LongSlit 1/1Page: Nov. 23, 2005. JSW

Date:

FILTER_SLIDE:_FILTER_2_(IN) S4

FILTER_SLIDE:_FILTER_1_(OUT) S3

FLIP_MIRROR:_FIELD/LAMP_VIEW S2

FLIP_MIRROR:_SLIT_VIEW S1

IMS#_M1716-1.5S

M1

PHOTRON#_P814A LP1

NTE#R56-7D.5-6D K1

CIRCULAR

4 PIN

J5

9 PIN D

J4

25 PIN D

J3

15 PIN D

J2

5 PIN HEXAGONAL

J1

24RET

24RET